Menu operation:

A001: DMX address setting

P015: Output fog volume setting

I060: timing pause time

O060: Timquantitative output time

Hidden menu (long press the first button to enter under the main interface)

H280: upper temperature limit

L200: Lower temperature limit

BOF: whether the backlight is automatically turned off after 60 seconds

The rON: control switch

The OON: oil-free detection switch

-005: Oil-free parameters

-OF-: Select ON and press the fourth key to restore the factory settings

Control operation (operation under the main interface):

First key: the menu key

The second button: spray smoke, display FOG when working

Third key: bubble, working display BUBB

The fourth key: cigarette bubble, working forward time

Control desk operation:

First channel: 10-255 output fog volume 1-100%

The second channel: 10-255 bubble output open 0-10 bubble output off

Third passage: 0-255 red light

Fourth channel: 0-255 green light

Channel 5:0-255 blue light

Channel 6: the light gradient, the larger the value, the faster the gradient

Seventh channel: light strobe, the larger the value, the faster the strobe

Shake control control:

Under the arrow: spray

On the arrow: bubble

Lock key: stop

Block: Fog bubble